<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="20" y1="18" x2="20" y2="2" width="0" layer="20"/>
<wire x1="20" y1="2" x2="18" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="18" y1="0" x2="2" y2="0" width="0" layer="20"/>
<wire x1="2" y1="0" x2="0" y2="2" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="2" x2="0" y2="18" width="0" layer="20"/>
<wire x1="20" y1="18" x2="18" y2="20" width="0" layer="20" curve="90"/>
<wire x1="0" y1="18" x2="2" y2="20" width="0" layer="20" curve="-90"/>
<wire x1="2" y1="20" x2="18" y2="20" width="0" layer="20"/>
<circle x="18" y="18" radius="1.143" width="0.0254" layer="20"/>
<circle x="18" y="2" radius="1.143" width="0.0254" layer="20"/>
<circle x="2" y="18" radius="1.143" width="0.0254" layer="20"/>
<circle x="2" y="2" radius="1.143" width="0.0254" layer="20"/>
<text>Crowtail- BME280</text>
<text>Atmospheric Sensor</text>
<text>www.elecrow.com</text>
<text>v1.0</text>
<text>I</text>
<text>SCL</text>
<text>SDA</text>
<text>VCC</text>
<text>GND</text>
</plain>
<libraries>
<library name="BME280ComponentLibrary">
<packages>
<package name="BME280_LGA">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="Discrete">
<packages>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="IC">
<packages>
<package name="SOT89">
<description>SOT98 Emitter Collector Basis</description>
</package>
</packages>
</library>
<library name="CONNECTER">
<packages>
<package name="2.0_1X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="BME280ComponentLibrary" package="BME280_LGA" value="BME280">
<attribute name="PROD_ID" value="IC-13090"/>
<attribute name="VALUE" value="BME280"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE" value="4.7K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE" value="4.7K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="4.7K">
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE" value="4.7K"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="Discrete" package="C0805" value="10UF/10V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="Discrete" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="Discrete" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="IC" package="SOT89" value="LD1117-3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="CONNECTER" package="2.0_1X4" value="TWIG_2.0">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="P$7"/>
<contactref element="U1" pad="P$1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="P$3"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="P$4"/>
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="C13" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="P$8"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="P$6"/>
<contactref element="C1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="SDO/ADR">
<contactref element="U1" pad="P$5"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
